| III. BOOT-51 Operation When BOOT-51 is customized correctly, and the target board is connected to the host PC with the cable(s) described above, we can start to upload and run application programs. There are two possible modes of operation: interactive operation batch operation Interactive Operation Batch File Operation under MS-DOS DOS Upload Utilities Shell Script Operation under Linux The BLINK Program