| III.10.2 IFxx and ELSEIFxx Instructions The particular IFxx instructions are working as follows:
IF <expr> | The IF condition is TRUE, if the expression <expr> is not equal to 0. The value of <expr> must be known on pass 1!
IFN <expr> | The IFN condition is TRUE, if the expression <expr> is equal to 0. The value of <expr> must be known on pass 1!
IFDEF <symbol> | The IFDEF condition is TRUE, if the <symbol> is defined in the program. Forward references to <symbol> are not allowed!
IFNDEF <symbol> | The IFNDEF condition is TRUE, if the <symbol> is not defined in the program. Forward references to <symbol> are not allowed!
IFB <literal> | The IFB (if blank) condition is TRUE, if the <literal> is empty. <literal> is a string, enclosed in angle brackets.
IFNB <literal> | The IFNB (if not blank) condition is TRUE, if the <literal> is not empty. <literal> is a string, enclosed in angle brackets.
| Although the IFB and IFNB statements are valid also outside of macros, they can be applied sensefully in macro bodies only. Usually they are used to decide, whether macro arguments have been left blank, or not.
The corresponding ELSEIFxx instructions are working respectively. Example 1: IF .. ELSE .. ENDIF construction
            TARGET EQU 0    ;configuration:  1 for application board
                            ;--------------  0 for evaluation board
            IF TARGET
              ORG 0         ;program start address of application board
            ELSE
              ORG 8000H     ;program start address of evaluation board
            ENDIF
Currently the program is configured for the evaluation board version. Example 2: IFNDEF .. ELSE .. ENDIF construction
           ;EVA_537 EQU 0     ;symbol undefined: 80C537 application board
                              ;symbol defined:   80C537 evaluation board
            IFNDEF EVA_537
              CLOCK EQU 16    ;clock frequency of application board
              CSEG  AT  0     ;program start address of application board
            ELSE
              CLOCK EQU 12    ;clock frequency of evaluation board
              CSEG  AT  8000H ;program start address of evaluation board
            ENDIF
Currently the program is configured for the application board version. Example 3: IFB .. ELSE .. ENDIF construction
            DECIDE MACRO X, Y
              IFB <X&Y>
                NOP
                NOP
              ELSE
                DB '&X,&Y'
              ENDIF
            ENDM
If the above macro is invoked as follows,
            DECIDE Nonsense
the parameter X will be replaced by "Nonsense" and the parameter Y by a zero length string. Thus the IFB literal becomes <Nonsense>, and the macro will be expanded to:
            DB 'Nonsense,'
If the macro will be invoked without arguments,
            DECIDE
the parameters X and Y will be replaced by zero length strings both, and the IFB literal becomes <>. Thus the macro will be expanded to:
            NOP
            NOP
Macros are explained in detail in chapter "III.11 Macro Processing". Example 4: IFNDEF .. ELSEIF .. ELSEIF .. ELSE .. ENDIF construction The symbol BAUDRATE serves to define the UART baudrate:
            IFNDEF BAUDRATE
              LJMP AUTOBAUD            ;automatic baudrate detection
            ELSEIF BAUDRATE EQ 9600
              MOV TH1, #0FDH           ;9600 baud
            ELSEIF BAUDRATE EQ 1200
              MOV TH1, #0E8H           ;1200 baud
            ELSE
              $ERROR(baudrate not implemented)
            ENDIF
If the symbol BAUDRATE is not defined at all, a jump to the label AUTOBAUD is performed. If the symbol BAUDRATE is defined with one of the legal values 9600 or 1200, timer 1 is initialized accordingly. If the symbol BAUDRATE is defined with another value, a corresponding user-defined error message is generated.