| II.1 Files The BOOT-51 package for DOS/Windows consists of the following files:
`BOOT51.DOC` |  | BOOT-51 User's Manual, ASCII format
`BOOT51.HTM` |  | index file of the BOOT-51 documentation, HTML format
`*.HTM` |  | further pages of the HTML documentation
`*.GIF` |  | GIF images referenced by HTML pages
`BOOT51.A51` |  | BOOT-51 assembler source (for ASEM-51 V1.3 and up)
`CUSTOMIZ.EXE` |  | BOOT-51 customization utility
`BOOT.BAT` |  | batch file for application program upload
`UPLOAD.BAT` |  | called by BOOT.BAT only
`COMPORT.EXE` |  | setup utility for PC serial ports
`RESET51.EXE` |  | program to reset target system via PC ports
`SLEEP.EXE` |  | program to wait for the reset recovery time
`BLINK.A51` |  | sample test program for BOOT-51
The BOOT-51 package for Linux consists of the following files:
`boot51.doc` |  | BOOT-51 User's Manual, ASCII format
`boot51.htm` |  | index file of the BOOT-51 documentation, HTML format
`*.htm` |  | further pages of the HTML documentation
`*.gif` |  | GIF images referenced by HTML pages
`boot51.a51` |  | BOOT-51 assembler source (for ASEM-51 V1.3 and up)
`customiz` |  | BOOT-51 customization utility
`customiz.1` |  | man-page for customiz
`boot` |  | shell script for application program upload
`boot.1` |  | man-page for boot
`upload` |  | called by boot only (generic version)
`upload.new` |  | "new" upload (optimized for stty 2.0 or later)
`reset51` |  | program to reset target system via PC ports
`reset51.1` |  | man-page for reset51
`blink.a51` |  | sample test program for BOOT-51